Bathtub Installation Instructions

There is more than one way to install your bathtub depending on if your tub will have an overflow. We recommend that bathtub installations are best handled by professionals, due to the precise plumbing involved.

1. Determine the desired location and orientation of the tub and mark the location on the floor using your copper bathtub.
2. Use a tape measure and mark the centerline of the drain location on the floor
3. Determine water line locations for selected bathtub filler.
4. Install the drain and optional overflow drains onto the bathtub as per the drain and overflow kit instruction
5. Place the bathtub in desired location and verify that the tub is level.
6. Run the drainpipes through the floor and attach to the plumbing.
7. Finish installation by running a bead of silicone adhesive around the base of copper freestanding bathtub. We recommend using a clear, acid free silicone such as a GEII (General Electric Roman numeral 2) silicone. You can find these items at your local hardware store or order them online.
8. Allow silicone to thoroughly dry before filling bathtub with water.
9. When cleaning up after installations, do not use abrasive cleaners.